**Day 29 Notes**

**Keep Day 28 CAD and Circuit**

**Then Rewire 7 Segment Display**

* const byte DISTANCE\_DISPLAY\_DIO\_PIN = 4;
* const byte DISTANCE\_DISPLAY\_CLK\_PIN = 5;


**Flight 1: Winner 100.121 sec**

**Flight 2: Winner 66.730 sec**

**Flight 3: Winner 82.348 sec**

**Flight 4: Crash – Too Tast (Speed Limit) 31.699 sec**

Example Circuit



**~~My Circuit (AS DRAWN)~~**

A circuit board with wires and wires

Description automatically generated

**My Circuit (AS Built)**

**A diagram of a circuit board

Description automatically generated**